**16/07/25**

This folder contains the plots comparing damage to several parameters. The damage and parameters are both calculated for every 10-minute interval and so the scatter graph has many points. The damage is always calculated with the measured distribution. The three parameters are:

* Rainfall [mm] of the 10 minute period
* Dmass [mm] of the 10 minute period, calculated with either the Best distribution, or directly from measurements.

The plots are on a log scale as otherwise trends are difficult to visualise.